**Episode 1**

In this video series we're going to look at setting up a home server using a Raspberry Pi 4 8GB. You can use other versions of the Pi 4, but I recommend the 8GB model as it is going to be our main server.

In this video we're going to take a look at the hardware I'm going to use in my Raspberry Pi Home Server:

- Raspberry Pi 4 8GB

- Argon One M.2 Case

- Silicon Power 256GB Boot Drive

- Sabrent 2TB Rocket NVMe PCIe M.2 Storage Drive

- Sabrent USB 3.2 Tool-Free NVMe Enclosure

Currently the Argon One M.2 case is NOT \*currently\* available on Amazon, but you can get it on their website: <https://dbte.ch/argononem2>​

AFFILIATE LINKS:

You can get their standard (non-M.2) Argon One case here: <https://amzn.to/3ouFtnx>​

Silicon Power 256GB A55 M.2 SSD: <https://amzn.to/2G00chM>​

Sabrent 2TB Rocket NVMe PCIe M.2: <https://amzn.to/3ovZmuv>​

Sabrent USB 3.2 Tool-Free NVMe Enclosure: <https://amzn.to/35xruVG>​

CanaKit Raspberry Pi 4 8GB: <https://amzn.to/2FZDvKA>​

**Episode 2**

I've been working on getting to a video about installing OpenMediaVault on a Raspberry Pi for a while now and even went so far as to download the files I would need for the video and put them on my desktop for safe keeping and a little reminder to hurry up and make the video.

This morning I decided to finally make the video. I went back through some online resources and realized they had changed the entire process when they released version 5 of OpenMediaVault.

Makes me glad that I didn't make that video sooner.

In order to setup an OpenMediaVault Raspberry Pi server, you're going to need a few things:

- Raspberry Pi 3 or 4 with a proper power supply

- Micro SD Card - 8GB or more with USB Adapter

- Ethernet Cable is preferable for network access

- External USB Hard Drive that you're okay formatting / erasing

- A Computer - I'm using a Windows 10 PC

- SSH program like Putty

Once you've gathered all that, you're set to go.

The rest of the instructions can be found here on my blog:

<https://dbte.ch/omv>

Now it’s time to work on making sure that Raspian is full updated. In the terminal window, type:

sudo apt-get update

Let the system complete. When you’ve got a blinking cursor, type the following:

sudo apt-get upgrade

This may take several minutes, so let it run until you get back to a blinking cursor. Then type:

sudo reboot

This will reboot your Raspberry Pi and close your Putty connection. Wait a couple of minutes and the open Putty and login like you did before with your new password.

Next, you’ll add the “pi” user to the SSH group with this command:

sudo adduser pi ssh

Once that’s complete, you’re going to download and execute a file from Github that will install and configure the OpenMediaVault server software. That script is this:

wget -O - https://github.com/OpenMediaVault-Plugin-Developers/installScript/raw/master/install | sudo bash

This process may take a while depending on your internet connection and what version Raspberry Pi you’ve got. It took me about 15 minutes to complete this, but understand that it could take upwards of 30 minutes.

Once the script has run and completed, reboot the Raspberry Pi:

sudo reboot

At this point, you can plug in your external USB hard drive.

**Episode 3**

Overclock Commands and entries

SSH into your Pi and run this command:

sudo nano /boot/config.txt

Then add these lines and save:

over\_voltage=2

arm\_freq=1750

gpu\_freq=750

RPi-Monitor Docker Container

SSH into your Pi and run this command:

docker run --device=/dev/vchiq --volume=/opt/vc:/opt/vc --volume=/boot:/boot --volume=/sys:/dockerhost/sys:ro --volume=/etc:/dockerhost/etc:ro --volume=/proc:/dockerhost/proc:ro --volume=/usr/lib:/dockerhost/usr/lib:ro -p=8888:8888 --name="rpi-monitor" -d michaelmiklis/rpi-monitor:latest

**Episode 4**

Here is the stack we'll use for Duplicati on our Raspberry Pi:

---

version: "2.1"

services:

duplicati:

image: linuxserver/duplicati

container\_name: duplicati

environment:

- PUID=998

- PGID=100

- TZ=America/Denver

volumes:

- /srv/dev-disk-by-label-Files/Config/Duplicati:/config #Config Files

- /srv/dev-disk-by-label-Files/Backups:/BackupStorage #Backup Storage

- /srv/dev-disk-by-label-Files/Config:/ConfigBackup #What to Backup

- /srv/dev-disk-by-label-Files/Databases:/DatabaseBackup #What to Backup

ports:

- 8200:8200

restart: unless-stopped

**Episode 5**

Once you’re logged in via SSH, create a folder called nginx and a new file called config.json in that folder:

mkdir nginx

cd nginx

nano config.json

Then you can paste the following into the terminal screen:

{

"database": {

"engine": "mysql",

"host": "db",

"name": "npm",

"user": "npm",

"password": "npm",

"port": 3306

}

}

Save and close the file.

Now you’ll create a file called docker-compose.yml:

nano docker-compose.yml

Then paste the following in the terminal screen:

---

version: '3'

services:

app:

image: 'jc21/nginx-proxy-manager:latest'

ports:

- '80:80' #HTTP Traffic

- '81:81' #Dashboard Port

- '443:443' #HTTPS Traffic

volumes:

- ./config.json:/app/config/production.json

- ./data:/data

- ./letsencrypt:/etc/letsencrypt

db:

image: 'jc21/mariadb-aria:10.4'

environment:

MYSQL\_ROOT\_PASSWORD: 'npm'

MYSQL\_DATABASE: 'npm'

MYSQL\_USER: 'npm'

MYSQL\_PASSWORD: 'npm'

volumes:

- ./data/mysql:/var/lib/mysql

Save and close the file.

Then, to deploy the new container, you can enter the following in your terminal:

sudo docker-compose up -d

Normally we wouldn’t run this as sudo, but there have been incidents where an error comes up about Docker being installed in a non-standard location and running this as sudo seems to get around that.

Once everything has deployed in the terminal screen, you can jump over to Portainer and take a look at the logs for the nginx\_app (or similarly named) and make sure that everything has completed.

If the last line of the logs is this:

Creating a new JWT key pair...

Then you need to wait a bit longer for things to finish up.

Once everything has finished, you can go to http://your-server-address:81

The default login credentials are:

Username: admin@example.com

Password: changeme

Once you’re logged in, you’ll be prompted to change the username and password.

That’s it! Now you’ve got NGINX Proxy Manager installed on a Raspberry Pi 4!

**CloudFlare DDNS - Update CloudFlare with Your Dynamic IP Address**

https://hub.docker.com/r/oznu/cloudflare-ddns

## Usage

Quick Setup:

docker run \

-e API\_KEY=xxxxxxx \

-e ZONE=example.com \

-e SUBDOMAIN=subdomain \

oznu/cloudflare-ddns

## Parameters

* --restart=always - ensure the container restarts automatically after host reboot.
* -e API\_KEY - Your CloudFlare scoped API token. See the [Creating a Cloudflare API token](https://hub.docker.com/r/oznu/cloudflare-ddns" \l "creating-a-cloudflare-api-token) below. Required
  + API\_KEY\_FILE - Path to load your CloudFlare scoped API token from (e.g. a Docker secret). If both API\_KEY\_FILE and API\_KEY are specified, API\_KEY\_FILE takes precedence.
* -e ZONE - The DNS zone that DDNS updates should be applied to. Required
* -e SUBDOMAIN - A subdomain of the ZONE to write DNS changes to. If this is not supplied the root zone will be used.

## Optional Parameters

* -e PROXIED - Set to true to make traffic go through the CloudFlare CDN. Defaults to false.
* -e RRTYPE=A - Set to AAAA to use set IPv6 records instead of IPv4 records. Defaults to A for IPv4 records.
* -e DELETE\_ON\_STOP - Set to true to have the dns record deleted when the container is stopped. Defaults to false.
* -e INTERFACE=tun0 - Set to tun0 to have the IP pulled from a network interface named tun0. If this is not supplied the public IP will be used instead. Requires --network host run argument.
* -e CUSTOM\_LOOKUP\_CMD="echo '1.1.1.1'" - Set to any shell command to run them and have the IP pulled from the standard output. Leave unset to use default IP address detection methods.
* -e DNS\_SERVER=10.0.0.2 - Set to the IP address of the DNS server you would like to use. Defaults to 1.1.1.1 otherwise.
* -e CRON="@daily" - Set your own custom CRON value before the exec portion. Defaults to every 5 minutes - \*/5 \* \* \* \*.

## Depreciated Parameters

* -e EMAIL - Your CloudFlare email address when using an Account-level token. This variable MUST NOT be set when using a scoped API token.

## Creating a Cloudflare API token

To create a CloudFlare API token for your DNS zone go to <https://dash.cloudflare.com/profile/api-tokens> and follow these steps:

1. Click Create Token
2. Provide the token a name, for example, cloudflare-ddns
3. Grant the token the following permissions:
   * Zone - Zone Settings - Read
   * Zone - Zone - Read
   * Zone - DNS - Edit
4. Set the zone resources to:
   * Include - All zones
5. Complete the wizard and copy the generated token into the API\_KEY variable for the container

## Multiple Domains

If you need multiple records pointing to your public IP address you can create CNAME records in CloudFlare.

## IPv6

If you're wanting to set IPv6 records set the envrionment variable RRTYPE=AAAA. You will also need to run docker with IPv6 support, or run the container with host networking enabled.

## Docker Compose

If you prefer to use [Docker Compose](https://docs.docker.com/compose/):

version: '2'

services:

cloudflare-ddns:

image: oznu/cloudflare-ddns:latest

restart: always

environment:

- API\_KEY=xxxxxxx

- ZONE=example.com

- SUBDOMAIN=subdomain

- PROXIED=false

## License

Copyright (C) 2017-2020 oznu

This program is free software: you can redistribute it and/or modify it under the terms of the GNU General Public License as published by the Free Software Foundation, either version 3 of the License, or (at your option) any later version.

This program is distributed in the hope that it will be useful, but WITHOUT ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the [GNU General Public License](https://hub.docker.com/r/oznu/LICENSE) for more details.

## Image Variants

| Image Tag | Architecture | OS | Size |
| --- | --- | --- | --- |
| latest | x64 | Alpine Linux |  |
| armhf | arm32v6 | Alpine Linux |  |
| aarch64 | arm64 | Alpine Linux |  |

**Episode 7**

### Installation

Open Portainer on your Raspberry Pi and create a new Stack.

Paste the following into your new stack:

version: '2'

volumes:

nextcloud:

db:

services:

db:

image: yobasystems/alpine-mariadb:latest

command: --transaction-isolation=READ-COMMITTED --binlog-format=ROW

restart: always

volumes:

- db:/var/lib/mysql

environment:

- MYSQL\_ROOT\_PASSWORD=password #Change This

- MYSQL\_PASSWORD=password #Change This

- MYSQL\_DATABASE=nextcloud

- MYSQL\_USER=nextcloud

app:

image: nextcloud

ports:

- 8080:80

links:

- db

volumes:

- nextcloud:/var/www/html #Change 'nextcloud' to your external drive volume if available

restart: always

Change the few things as noted above.

Click the “Deploy the Stack” button.

Next, go to your NGINX Proxy Manager dashboard. Create a new Proxy Host.

* Fill in the domain name (or subdomain) you designated for your NextCloud install.
* Scheme should be http.
* Forward Hostname/IP should be your Raspberry Pi’s IP address.
* Foward port should be 8080.
* Click the “Block Common Exploits” toggle.

Go to the SSL tab.

* Change “None” to “Request a New SSL Certificate”.
* Click the “Force SSL” and “HTTP/2 Support” toggles.
* You can click the HSTS toggles if you’ve enabled HSTS in CloudFlare.
* Click “Save”.

After a moment, you should see that everything has deployed correctly.

Next, go to [https://nextcloud.yourdomain.com](https://nextcloud.yourdomain.com/) (change this to your actual domain) and you should see the NextCloud install page.

* Enter an Admin username and password.
* Change the database type to MySQL/MariaDB.
* Enter the username, password, and database name as you have them in your Portainer Stack.
* Change Database location to from “localhost” to “db” (without quotes).
* Toggle the option for additional app installation to meet your needs.
* Click “Finish setup”.

At this point, you can go get some lunch or something as the install process will take a while since we’re on a 4 core ARM processor.

Once the install is complete, you’ll be taken to the NextCloud dashboard and then you should be good to go!

**Episode 8**

<https://gist.github.com/dnburgess/40c2b297911d1de4353f74c3da8f951f>

DB Tech BitWardenRS on Pi 4

[gistfile1.txt](https://gist.github.com/dnburgess/40c2b297911d1de4353f74c3da8f951f" \l "file-gistfile1-txt)

---

version: "2"

services:

bitwardenrs:

image: bitwardenrs/server:latest

container\_name: bitwardenrs

volumes:

- /srv/dev-disk-by-label-Files/Config/BitWardenRS:/data/

ports:

- 8100:80

restart: unless-stopped

### Prerequisites

You’ll need to have Traefik and CloudFlare setup for this to work. Check out this tutorial in order to get that setup: <https://dbtechreviews.com/2020/04/how-to-install-traefik-on-omv-and-docker/>

Bitwarden will NOT let you access its vault unless you’re accessing it on an https:// URL.

### Installation of Bitwarden

You can find a [basic SSH command](https://bitwarden.com/" \l "host-it-yourself) to run on Bitwarden’s website, but we’re not going to use that since we like to use Stacks whenever possible.

Here’s the Stack that we’re going to use for this installation:

---

version: "2"

services:

bitwarden:

image: bitwardenrs/server:latest

container\_name: bitwarden

labels:

- traefik.enable=true

- traefik.http.routers.bitwarden.rule=Host(`pw.dbtechdemo.com`)

- traefik.http.routers.bitwarden.entrypoints=web

- traefik.http.services.bitwarden.loadbalancer.server.port=80

networks:

- web

volumes:

- /srv/dev-disk-by-label-Files/Config/BitWarden:/data/

restart: unless-stopped

The only things you should need to change here is the URL used to access Bitwarden and the location of your Config folder in volumes. Once you have those 2 things changed to fit your setup, you can click the “Deploy the Container” button and give it a few minutes to download and setup everything needed for Bitwarden.

# How to Install Traefik on OMV and Docker

Traefik is the leading open source reverse proxy and load balancer for HTTP and TCP-based applications that is easy, dynamic, automatic, fast, full-featured, production proven, provides metrics, and integrates with every major cluster technology… No wonder it’s so popular!

Setting up Traefik is super simple, but, because it uses a version 3 Stack, we can’t do this in Portainer. That means we’ll have to do it in an SSH program like PuTTY.

### Setting Up Your Domain Name

In order to set this up, you’ll need to have a domain name available that you can use to point to your home’s IP address. We’re going to use [CloudFlare](https://www.cloudflare.com/) to do this as it will do a couple of really important things:

* 1. It will give us the SSLs we need to secure the traffic on our domain.
  2. It will mask our home IP address, so if someone finds your domain name and they ping it, they will get a CloudFlare IP address and not your home’s IP address.
  3. It will also help block malicious traffic trying to hit your server. It won’t be perfect, but it will do a lot of blocking for you.

### Installing Traefik

First thing is to open Portainer and go to the Network tab. Once there, create a new network called “web” (without the quotes) and leave it set as a bridge network.

Next, open PuTTY and connect to your server on port 22 as root.

In the directory you landed on when you logged in, enter the following commands to create and move into a folder called traefik:

mkdir traefik

cd traefik

Next, you’ll need to create a couple of files. First, we’ll create a file called dynamic.yaml:

nano dynamic.yaml

Press return on your keyboard and copy/paste the following into the mostly empty screen:

## Setting up the middleware for redirect to https ##

http:

middlewares:

redirect:

redirectScheme:

scheme: https

Then press CTRL+O and then Enter to save the file. Then press CTRL+X to exit the file.

The next file we’ll create is docker-compose.yml:

nano docker-compose.yml

Press return on your keyboard and copy/paste the following into the mostly empty screen:

version: "3.3"

services:

traefik:

image: traefik:v2.0

restart: always

container\_name: traefik

ports:

- "80:80" # <== http

- "8080:8080" # <== :8080 is where the dashboard runs on

- "443:443" # <== https

command:

- --api.insecure=true # <== Enabling insecure api, NOT RECOMMENDED FOR PRODUCTION

- --api.dashboard=true # <== Enabling the dashboard to view services, middlewares, routers, etc...

- --api.debug=true # <== Enabling additional endpoints for debugging and profiling

- --log.level=DEBUG # <== Setting the level of the logs from traefik

- --providers.docker=true # <== Enabling docker as the provider for traefik

- --providers.docker.exposedbydefault=false # <== Don't expose every container to traefik, only expose enabled ones

- --providers.file.filename=/dynamic.yaml # <== Referring to a dynamic configuration file

- --providers.docker.network=web # <== Operate on the docker network named web

- --entrypoints.web.address=:80 # <== Defining an entrypoint for port :80 named web

volumes:

- /var/run/docker.sock:/var/run/docker.sock # <== Volume for docker admin

- ./dynamic.yaml:/dynamic.yaml # <== Volume for dynamic conf file, \*\*ref: line 27

networks:

- web # <== Placing traefik on the network named web, to access containers on this network

labels:

- "traefik.enable=true" # <== Enable traefik on itself to view dashboard and assign subdomain to view it

- "traefik.http.routers.api.rule=Host(`monitor.dbtechdemo.com`)" # <== Setting the domain for the dashboard

- "traefik.http.routers.api.service=api@internal" # <== Enabling the api to be a service to access

networks:

web:

external: true

Change the URL of [monitor.dbtechdemo.com](http://monitor.dbtechdemo.com/) to whatever your monitor URL will be.

Then press CTRL+O and then Enter to save the file. Then press CTRL+X to exit the file.

Now that you’ve created the files you’ll need, you can enter the following command:

docker-compose up -d

The script will run and should only take a minute to complete. Once it has completed, head back to Portainer to look at the logs for the Traefik container.

Once things have settled down, you can go to [http://your-server-ip:8080](http://your-server-ip:8080/) and see the Traefik dashboard.

**Episode 9**

DB Tech Pi-hole on Pi 4

[gistfile1.txt](https://gist.github.com/dnburgess/5caf8ff10f65bdc2467d532f55753774" \l "file-gistfile1-txt)

---

version: 2

services:

pihole:

container\_name: pihole

image: pihole/pihole:latest

ports:

- 53:53/tcp #DNS Port

- 53:53/udp #DNS Port

#- 67:67/udp #DHCP Port

- 83:80/tcp #Dashboard Port

#- 443:443/tcp #Port 443 is to provide a sinkhole for ads that use SSL.

environment:

TZ: America/Denver

WEBPASSWORD: password

DNS1: 1.1.1.1

DNS2: 1.0.0.1

DNSSEC: 'true'

volumes:

- /srv/dev-disk-by-label-Files/Config/Pihole/etc-pihole/:/etc/pihole/

- /srv/dev-disk-by-label-Files/Config/Pihole/etc-dnsmasq.d/:/etc/dnsmasq.d/

cap\_add:

- NET\_ADMIN

restart: unless-stopped

This won't work out of the box as Raspbian has port 53 being used. We need to stop and reconfigure the service using it.

To stop systemd-resolved, run this command:

sudo systemctl stop systemd-resolved

To edit systemd-resolved, run this command:

sudo nano /etc/systemd/resolved.conf

Edit the file so it looks like this:

[Resolve]

DNS=1.1.1.1

FallbackDNS=1.0.0.1

#Domains=

#LLMNR=yes

#MulticastDNS=yes

#DNSSEC=allow-downgrade

#DNSOverTLS=no

#Cache=yes

#DNSStubListener=yes

#ReadEtcHosts=yes

DNSStubListener=no

Save and exit.

To create a symlink of the changes you made, run this command:

sudo ln -sf /run/systemd/resolve/resolv.conf /etc/resolv.conf

**Episode 10**

DB Tech WatchTower on Pi 4

version: '2.1'

services:

watchtower:

image: containrrr/watchtower

container\_name: watchtower

volumes:

- /var/run/docker.sock:/var/run/docker.sock

environment:

- TZ=America/Denver

- WATCHTOWER\_MONITOR\_ONLY=true

- WATCHTOWER\_SCHEDULE=0 0 16 ? \* THU

- WATCHTOWER\_CLEANUP=true

- WATCHTOWER\_NOTIFICATIONS=email

- WATCHTOWER\_NOTIFICATION\_EMAIL\_FROM=FromEmail@gmail.com

- WATCHTOWER\_NOTIFICATION\_EMAIL\_TO=ToEmail@gmail.com

- WATCHTOWER\_NOTIFICATION\_EMAIL\_SERVER=smtp.gmail.com

- WATCHTOWER\_NOTIFICATION\_EMAIL\_SERVER\_PASSWORD=password

- WATCHTOWER\_NOTIFICATION\_EMAIL\_SUBJECTTAG=Pi Server Container Updates

- WATCHTOWER\_NOTIFICATION\_EMAIL\_SERVER\_USER=FromEmail@gmail.com

- WATCHTOWER\_NOTIFICATION\_EMAIL\_SERVER\_PORT=587

restart: unless-stopped

## **arguments.md**

By default, watchtower will monitor all containers running within the Docker daemon to which it is pointed (in most cases this will be the local Docker daemon, but you can override it with the --host option described in the next section). However, you can restrict watchtower to monitoring a subset of the running containers by specifying the container names as arguments when launching watchtower.

$ docker run -d \

--name watchtower \

-v /var/run/docker.sock:/var/run/docker.sock \

containrrr/watchtower \

nginx redis

In the example above, watchtower will only monitor the containers named "nginx" and "redis" for updates -- all of the other running containers will be ignored. If you do not want watchtower to run as a daemon you can pass the --run-once flag and remove the watchtower container after its execution.

$ docker run --rm \

-v /var/run/docker.sock:/var/run/docker.sock \

containrrr/watchtower \

--run-once \

nginx redis

In the example above, watchtower will execute an upgrade attempt on the containers named "nginx" and "redis". Using this mode will enable debugging output showing all actions performed, as usage is intended for interactive users. Once the attempt is completed, the container will exit and remove itself due to the --rm flag.

When no arguments are specified, watchtower will monitor all running containers.

## Help

Shows documentation about the supported flags.

Argument: --help

Environment Variable: N/A

Type: N/A

Default: N/A

## Time Zone

Sets the time zone to be used by WatchTower's logs and the optional Cron scheduling argument (--schedule). If this environment variable is not set, Watchtower will use the default time zone: UTC. To find out the right value, see [this list](https://en.wikipedia.org/wiki/List_of_tz_database_time_zones), find your location and use the value in TZ Database Name, e.g Europe/Rome. The timezone can alternatively be set by volume mounting your hosts /etc/timezone file. -v /etc/timezone:/etc/timezone:ro

Argument: N/A

Environment Variable: TZ

Type: String

Default: "UTC"

## Cleanup

Removes old images after updating. When this flag is specified, watchtower will remove the old image after restarting a container with a new image. Use this option to prevent the accumulation of orphaned images on your system as containers are updated.

Argument: --cleanup

Environment Variable: WATCHTOWER\_CLEANUP

Type: Boolean

Default: false

## Remove attached volumes

Removes attached volumes after updating. When this flag is specified, watchtower will remove all attached volumes from the container before restarting with a new image. Use this option to force new volumes to be populated as containers are updated.

Argument: --remove-volumes

Environment Variable: WATCHTOWER\_REMOVE\_VOLUMES

Type: Boolean

Default: false

## Debug

Enable debug mode with verbose logging.

Argument: --debug, -d

Environment Variable: WATCHTOWER\_DEBUG

Type: Boolean

Default: false

## Trace

Enable trace mode with very verbose logging. Caution: exposes credentials!

Argument: --trace

Environment Variable: WATCHTOWER\_TRACE

Type: Boolean

Default: false

## ANSI colors

Disable ANSI color escape codes in log output.

Argument: --no-color

Environment Variable: NO\_COLOR

Type: Boolean

Default: false

## Docker host

Docker daemon socket to connect to. Can be pointed at a remote Docker host by specifying a TCP endpoint as "tcp://hostname:port".

Argument: --host, -H

Environment Variable: DOCKER\_HOST

Type: String

Default: "unix:///var/run/docker.sock"

## Docker API version

The API version to use by the Docker client for connecting to the Docker daemon. The minimum supported version is 1.24.

Argument: --api-version, -a

Environment Variable: DOCKER\_API\_VERSION

Type: String

Default: "1.24"

## Include restarting

Will also include restarting containers.

Argument: --include-restarting

Environment Variable: WATCHTOWER\_INCLUDE\_RESTARTING

Type: Boolean

Default: false

## Include stopped

Will also include created and exited containers.

Argument: --include-stopped

Environment Variable: WATCHTOWER\_INCLUDE\_STOPPED

Type: Boolean

Default: false

## Revive stopped

Start any stopped containers that have had their image updated. This argument is only usable with the --include-stopped argument.

Argument: --revive-stopped

Environment Variable: WATCHTOWER\_REVIVE\_STOPPED

Type: Boolean

Default: false

## Poll interval

Poll interval (in seconds). This value controls how frequently watchtower will poll for new images. Either --schedule or a poll interval can be defined, but not both.

Argument: --interval, -i

Environment Variable: WATCHTOWER\_POLL\_INTERVAL

Type: Integer

Default: 86400 (24 hours)

## Filter by enable label

Update containers that have a com.centurylinklabs.watchtower.enable label set to true.

Argument: --label-enable

Environment Variable: WATCHTOWER\_LABEL\_ENABLE

Type: Boolean

Default: false

## Filter by disable label

Do not update containers that have com.centurylinklabs.watchtower.enable label set to false and no --label-enable argument is passed. Note that only one or the other (targeting by enable label) can be used at the same time to target containers.

## Without updating containers

Will only monitor for new images, send notifications and invoke the [pre-check/post-check hooks](https://containrrr.dev/watchtower/lifecycle-hooks/), but will not update the containers.

 Please note

Due to Docker API limitations the latest image will still be pulled from the registry.

Argument: --monitor-only

Environment Variable: WATCHTOWER\_MONITOR\_ONLY

Type: Boolean

Default: false

Note that monitor-only can also be specified on a per-container basis with the com.centurylinklabs.watchtower.monitor-only label set on those containers.

## Without restarting containers

Do not restart containers after updating. This option can be useful when the start of the containers is managed by an external system such as systemd.

Argument: --no-restart

Environment Variable: WATCHTOWER\_NO\_RESTART

Type: Boolean

Default: false

## Without pulling new images

Do not pull new images. When this flag is specified, watchtower will not attempt to pull new images from the registry. Instead it will only monitor the local image cache for changes. Use this option if you are building new images directly on the Docker host without pushing them to a registry.

Argument: --no-pull

Environment Variable: WATCHTOWER\_NO\_PULL

Type: Boolean

Default: false

## Without sending a startup message

Do not send a message after watchtower started. Otherwise there will be an info-level notification.

Argument: --no-startup-message

Environment Variable: WATCHTOWER\_NO\_STARTUP\_MESSAGE

Type: Boolean

Default: false

## Run once

Run an update attempt against a container name list one time immediately and exit.

Argument: --run-once

Environment Variable: WATCHTOWER\_RUN\_ONCE

Type: Boolean

Default: false

## HTTP API Mode

Runs Watchtower in HTTP API mode, only allowing image updates to be triggered by an HTTP request. For details see [HTTP API](https://containrrr.github.io/watchtower/http-api-mode).

Argument: --http-api-update

Environment Variable: WATCHTOWER\_HTTP\_API

Type: Boolean

Default: false

## HTTP API Token

Sets an authentication token to HTTP API requests.

Argument: --http-api-token

Environment Variable: WATCHTOWER\_HTTP\_API\_TOKEN

Type: String

Default: -

## Filter by scope

Update containers that have a com.centurylinklabs.watchtower.scope label set with the same value as the given argument. This enables [running multiple instances](https://containrrr.github.io/watchtower/running-multiple-instances).

Argument: --scope

Environment Variable: WATCHTOWER\_SCOPE

Type: String

Default: -

## HTTP API Metrics

Enables a metrics endpoint, exposing prometheus metrics via HTTP. See [Metrics](https://github.com/containrrr/watchtower/blob/master/docs/metrics.md) for details.

Argument: --http-api-metrics

Environment Variable: WATCHTOWER\_HTTP\_API\_METRICS

Type: Boolean

Default: false

## Scheduling

[Cron expression](https://pkg.go.dev/github.com/robfig/cron@v1.2.0?tab=doc" \l "hdr-CRON_Expression_Format) in 6 fields (rather than the traditional 5) which defines when and how often to check for new images. Either --interval or the schedule expression can be defined, but not both. An example: --schedule "0 0 4 \* \* \*"

Argument: --schedule, -s

Environment Variable: WATCHTOWER\_SCHEDULE

Type: String

Default: -

## Rolling restart

Restart one image at time instead of stopping and starting all at once. Useful in conjunction with lifecycle hooks to implement zero-downtime deploy.

Argument: --rolling-restart

Environment Variable: WATCHTOWER\_ROLLING\_RESTART

Type: Boolean

Default: false

## Wait until timeout

Timeout before the container is forcefully stopped. When set, this option will change the default (10s) wait time to the given value. An example: --stop-timeout 30s will set the timeout to 30 seconds.

Argument: --stop-timeout

Environment Variable: WATCHTOWER\_TIMEOUT

Type: Duration

Default: 10s

## TLS Verification

Use TLS when connecting to the Docker socket and verify the server's certificate. See below for options used to configure notifications.

Argument: --tlsverify

Environment Variable: DOCKER\_TLS\_VERIFY

Type: Boolean

Default: false

**Episode 11**

**How To Setup MacVLAN in Portainer**

Information Not Found !!!

**Episode 12**

AdGuard Home is a network-wide software for blocking ads & tracking. After you set it up, it’ll cover ALL your home devices, and you don’t need any client-side software for that. With the rise of Internet-Of-Things and connected devices, it becomes more and more important to be able to control your whole network.

Instructions

First, create 2 volumes:

docker volume create agwork

docker volume create agconf

Next create the MacVLAN:

sudo docker network create -d macvlan -o parent=eth0 --subnet=192.168.68.0/24 --gateway=192.168.68.1 --ip-range=192.168.68.150/32 ag\_hal

IP Prefix Chart: https://www.ripe.net/images/IPv4CIDRChart\_2015.jpg

You'll most likely need to change the subnet to match your network's subnet. Also be sure to put in your router's IP address and change the IP range to match your network. You can change "ag\_hal" to whatever you want to name your MacVLAN.

Next run this command:

docker run --name adguardhome -v agwork:/opt/adguardhome/work -v agconf:/opt/adguardhome/conf -p 53:53/tcp -p 53:53/udp -p 67:67/udp -p 68:68/tcp -p 68:68/udp -p 80:80/tcp -p 443:443/tcp -p 853:853/tcp -p 3000:3000/tcp -d adguard/adguardhome

The command will fail and that's fine. Go to Portainer and edit the AdGuard container. Change the network from "bridge" to whatever you named your MacVLAN. Deploy the container.

Next, go to http://[your-macvlan-ip]:3000 and follow the setup instructions.

When that's done, you can login to your new AdGuard container by going to http://[your-macvlan-ip].

From there, you can customize the blocklists and that sort of thing to your liking.

**Episode 13**

DB Tech Transmission OpenVPN

version: 2

services:

transmission-openvpn:

volumes:

- /srv/dev-disk-by-label-Files/Torrents:/data

environment:

- OPENVPN\_PROVIDER=PIA

- OPENVPN\_CONFIG=France

- OPENVPN\_USERNAME=username

- OPENVPN\_PASSWORD=password

- WEBPROXY\_ENABLED=false

- LOCAL\_NETWORK=192.168.68.0/24

cap\_add:

- NET\_ADMIN

logging:

driver: json-file

options:

max-size: 10m

ports:

- 9091:9091

image: haugene/transmission-openvpn:latest-armhf

**Episode 14**

**OpenMediaVault: Setting Up Remote Mounts**

Null text information !!!

**Episode 15**

I took out port 443 as we'll be accessing this locally without SSL.

## Supported Architectures

Our images support multiple architectures such as x86-64, arm64 and armhf. We utilise the docker manifest for multi-platform awareness. More information is available from docker [here](https://github.com/docker/distribution/blob/master/docs/spec/manifest-v2-2.md" \l "manifest-list) and our announcement [here](https://blog.linuxserver.io/2019/02/21/the-lsio-pipeline-project/).

Simply pulling ghcr.io/linuxserver/heimdall should retrieve the correct image for your arch, but you can also pull specific arch images via tags.

The architectures supported by this image are:

| Architecture | Tag |
| --- | --- |
| x86-64 | amd64-latest |
| arm64 | arm64v8-latest |
| armhf | arm32v7-latest |

## Version Tags

This image provides various versions that are available via tags. latest tag usually provides the latest stable version. Others are considered under development and caution must be exercised when using them.

| Tag | Description |
| --- | --- |
| latest | Stable Heimdall releases. |
| development | Latest commit from the github master branch. |

## Usage

Here are some example snippets to help you get started creating a container.

### docker-compose ([recommended](https://docs.linuxserver.io/general/docker-compose))

Compatible with docker-compose v2 schemas.

---

version: "2.1"

services:

heimdall:

image: ghcr.io/linuxserver/heimdall

container\_name: heimdall

environment:

- PUID=1000

- PGID=1000

- TZ=Europe/London

volumes:

- </path/to/appdata/config>:/config

ports:

- 80:80

- 443:443

restart: unless-stopped

### docker cli

docker run -d \

--name=heimdall \

-e PUID=1000 \

-e PGID=1000 \

-e TZ=Europe/London \

-p 80:80 \

-p 443:443 \

-v </path/to/appdata/config>:/config \

--restart unless-stopped \

ghcr.io/linuxserver/heimdall

## Parameters

Container images are configured using parameters passed at runtime (such as those above). These parameters are separated by a colon and indicate <external>:<internal> respectively. For example, -p 8080:80 would expose port 80 from inside the container to be accessible from the host's IP on port 8080 outside the container.

| Parameter | Function |
| --- | --- |
| -p 80 | http gui |
| -p 443 | https gui |
| -e PUID=1000 | for UserID - see below for explanation |
| -e PGID=1000 | for GroupID - see below for explanation |
| -e TZ=Europe/London | Specify a timezone to use EG Europe/London |
| -v /config | Contains all relevant configuration files. |

## Environment variables from files (Docker secrets)

You can set any environment variable from a file by using a special prepend FILE\_\_.

As an example:

-e FILE\_\_PASSWORD=/run/secrets/mysecretpassword

Will set the environment variable PASSWORD based on the contents of the /run/secrets/mysecretpassword file.

## Umask for running applications

For all of our images we provide the ability to override the default umask settings for services started within the containers using the optional -e UMASK=022 setting. Keep in mind umask is not chmod it subtracts from permissions based on it's value it does not add. Please read up [here](https://en.wikipedia.org/wiki/Umask) before asking for support.

## User / Group Identifiers

When using volumes (-v flags) permissions issues can arise between the host OS and the container, we avoid this issue by allowing you to specify the user PUID and group PGID.

Ensure any volume directories on the host are owned by the same user you specify and any permissions issues will vanish like magic.

In this instance PUID=1000 and PGID=1000, to find yours use id user as below:

$ id username

uid=1000(dockeruser) gid=1000(dockergroup) groups=1000(dockergroup)

## Application Setup

Access the web gui at http://SERVERIP:PORT

### Adding password protection

This image now supports password protection through htpasswd. Run the following command on your host to generate the htpasswd file docker exec -it heimdall htpasswd -c /config/nginx/.htpasswd <username>. Replace /config/nginx/site-confs/default and restart the container after updating the image. A new site config with htpasswd support will be created in its place.

## Docker Mods

[](https://mods.linuxserver.io/?mod=heimdall) [](https://mods.linuxserver.io/?mod=universal)

We publish various [Docker Mods](https://github.com/linuxserver/docker-mods) to enable additional functionality within the containers. The list of Mods available for this image (if any) as well as universal mods that can be applied to any one of our images can be accessed via the dynamic badges above.

## Support Info

* Shell access whilst the container is running: docker exec -it heimdall /bin/bash
* To monitor the logs of the container in realtime: docker logs -f heimdall
* container version number
  + docker inspect -f '{{ index .Config.Labels "build\_version" }}' heimdall
* image version number
  + docker inspect -f '{{ index .Config.Labels "build\_version" }}' ghcr.io/linuxserver/heimdall

## Updating Info

Most of our images are static, versioned, and require an image update and container recreation to update the app inside. With some exceptions (ie. nextcloud, plex), we do not recommend or support updating apps inside the container. Please consult the [Application Setup](https://hub.docker.com/r/linuxserver/heimdall" \l "application-setup) section above to see if it is recommended for the image.

Below are the instructions for updating containers:

### Via Docker Compose

* Update all images: docker-compose pull
  + or update a single image: docker-compose pull heimdall
* Let compose update all containers as necessary: docker-compose up -d
  + or update a single container: docker-compose up -d heimdall
* You can also remove the old dangling images: docker image prune

### Via Docker Run

* Update the image: docker pull ghcr.io/linuxserver/heimdall
* Stop the running container: docker stop heimdall
* Delete the container: docker rm heimdall
* Recreate a new container with the same docker run parameters as instructed above (if mapped correctly to a host folder, your /config folder and settings will be preserved)
* You can also remove the old dangling images: docker image prune

### Via Watchtower auto-updater (only use if you don't remember the original parameters)

* Pull the latest image at its tag and replace it with the same env variables in one run:

docker run --rm \

-v /var/run/docker.sock:/var/run/docker.sock \

containrrr/watchtower \

--run-once heimdall

* You can also remove the old dangling images: docker image prune

Note: We do not endorse the use of Watchtower as a solution to automated updates of existing Docker containers. In fact we generally discourage automated updates. However, this is a useful tool for one-time manual updates of containers where you have forgotten the original parameters. In the long term, we highly recommend using [Docker Compose](https://docs.linuxserver.io/general/docker-compose).

### Image Update Notifications - Diun (Docker Image Update Notifier)

* We recommend [Diun](https://crazymax.dev/diun/) for update notifications. Other tools that automatically update containers unattended are not recommended or supported.

## Building locally

If you want to make local modifications to these images for development purposes or just to customize the logic:

git clone https://github.com/linuxserver/docker-heimdall.git

cd docker-heimdall

docker build \

--no-cache \

--pull \

-t ghcr.io/linuxserver/heimdall:latest .

The ARM variants can be built on x86\_64 hardware using multiarch/qemu-user-static

docker run --rm --privileged multiarch/qemu-user-static:register --reset

Once registered you can define the dockerfile to use with -f Dockerfile.aarch64.

**Episode 16**

[Here is the stack I used in this video that works](https://gist.github.com/dnburgess/1a9318cdeb4eb65ec0f50f6d024e8db7)

DB Tech Plex Temp Fix for Latest Release Issues

---

version: "2.1"

services:

plex:

image: ghcr.io/linuxserver/plex:1.21.0.3616-d87012962-ls5

container\_name: plex

network\_mode: host

environment:

- PUID=1000

- PGID=1000

- VERSION=docker

- UMASK\_SET=022 #optional

- PLEX\_CLAIM= #optional

volumes:

- /path/to/library:/config

- /path/to/tvseries:/tv

- /path/to/movies:/movies

restart: unless-stopped

[Here is a stack with the "bionic" tag](https://gist.github.com/dnburgess/081e8602b684c18d90c2c8aa6c750354)

DB Tech Plex Bionic Fix for Latest Release Issues

---

version: "2.1"

services:

plex:

image: ghcr.io/linuxserver/plex:bionic

container\_name: plex

network\_mode: host

environment:

- PUID=1000

- PGID=1000

- VERSION=docker

- UMASK\_SET=022 #optional

- PLEX\_CLAIM= #optional

volumes:

- /path/to/library:/config

- /path/to/tvseries:/tv

- /path/to/movies:/movies

restart: unless-stopped

**Episode 17**

**OpenMediaVault Recovery - OMV First Aid**

You can change your:

- OMV IP Address

- OMV Dashboard Port

- Change/Reset Your OMV Password

**Episode 18**

[WordPress Gist](https://gist.github.com/dnburgess/948d9c61199392db74742dc1aa99cea2)

DB Tech WordPress for Pi Home Server

version: '2.1'

services:

wordpress:

image: wordpress

restart: always

ports:

- 84:80

environment:

WORDPRESS\_DB\_HOST: db

WORDPRESS\_DB\_USER: exampleuser

WORDPRESS\_DB\_PASSWORD: examplepass

WORDPRESS\_DB\_NAME: exampledb

volumes:

- /srv/dev-disk-by-label-Files/Config/WordPress:/var/www/html

links:

- db:db

db:

image: yobasystems/alpine-mariadb:latest

restart: always

environment:

MYSQL\_DATABASE: exampledb

MYSQL\_USER: exampleuser

MYSQL\_PASSWORD: examplepass

MYSQL\_RANDOM\_ROOT\_PASSWORD: '1'

volumes:

- /srv/dev-disk-by-label-Files/Databases/WordPress:/var/lib/mysql

[Increase Memory Limit](https://victorthemes.com/increase-memory-wordpress-php-ini/)

# How To Increase Memory in WordPress PHP.ini Easily By Yourself

The uploaded file exceeds the upload\_max\_filesize directive in php.ini

You might be searching for result for the above error message and might be wondering how to increase memory in the php.ini WordPress website file. The following solution will help you fix the error within few minutes without waiting for the support team to answer you.

## Basic Commands You Need To Know

Before setting up to increase memory in WordPress php.ini we need to know what are the code we are going to use and what their functions are

### memory\_limit

The maximum amount of memory a script may consume, remember that the value you give here should be greater than your file size. For example, say that it is your memory card or disk space limit.

### max\_execution\_time

The execution time for each script. That is the time the server react to the file. For example, the time limit the server gate will be opened for your files to get into the server. If your file size is greater that cannot be uploaded in seconds then increase this

Sometimes this may also be one of the reason for getting the memory exhaust limit error and the server timed out message.

### post\_max\_size

Maximum size of POST data that PHP will accept. To disable the limit set it as zero. The POST request is a method requests that a web server accept the data enclosed in the body of the request message

### upload\_max\_filesize

Maximum allowed size in the server, this is the key for our increase memory in WordPress php.ini. You might have seen in your WordPress gallery that maximum upload size of the post or image.It defines the file size limit for a single file that you can upload to the server. It is one of the

It defines the file size limit for a single file that you can upload to the server. It is one of the method you can define to manage your space effectively on the server. This command will help you fix the memory limit exhaust problem in most cases.

## Ways To Increase Memory in WordPress



Mostly the memory exhausted error is caused from the server side not by your theme or by your network speed. Of course, the latter two may also cause trouble but the scenario is very rare. Saying that in order to fix this server side error we need to get your website’s server access.

For that first you have to log into your cpanel or your server account. Locate the WordPress root directory that is the folder location where your WordPress is installed. Once you have reached there your WordPress directory will be like this.

From here you can increase your memory by various methods as follows

### Create or Edit an existing PHP.INI file

Get into the wp-admin file and look for the php.ini or php5.ini. If there is one you have to edit it. If there is no such file in the wp-admin file then create a new folder named php.ini



After you have created the file copy the code below, paste it in the php.ini file and save it.

Pro Tip : all the values given are arbitrary value, change the values as per your need

upload\_max\_filesize = 720M  
post\_max\_size = 64M  
memory\_limit = 1024M  
max\_execution\_time = 180

If you are editing the existing php.ini file search for the term and change the value you need.

Pro Tip : to set the max post size without any limit use value 0 (zero)

This is the most common method you have to use to increase memory in WordPress php.ini

Note : Sometimes the hosting provider won’t let you have the access of the php.ini file or let the WordPress php.ini file to make any changes. If that is the case then we have to get the support from the server side only.

But still, you can try other methods mentioned below before reaching for the support.

### htaccess Method

htaccess is the next predominant way used by people to increase the memory limit or maximize the file upload size. In the directory, you can find the .htaccess file get into the file and paste the code below.

php\_value upload\_max\_filesize = 720M  
php\_value post\_max\_size = 64M  
php\_value memory\_limit = 1024M  
php\_value max\_execution\_time = 180

### Using wp-config.php file

The easiest method you can try and the probability of getting the issue fixed is also very low. Yet it is worth giving it a try. In your server search for wp-config.php file and paste the following code to increase the memory.

[code language=”PHP”]define( ‘WP\_MEMORY\_LIMIT’, ‘256M’ )[/code]

### Theme Functions File

The upload size can be sometimes can be fixed right from your theme function file itself. Again the probability of fixing this method is less. Copy and paste the following code in your functions.php file

@ini\_set( ‘upload\_max\_size’ , ‘720M’ );

@ini\_set( ‘post\_max\_size’, ’64M’);

@ini\_set( ‘max\_execution\_time’, ‘180’ );

## In the Popular Hosting Providers

Let us see how to Increase Upload Max File Size in PHP.ini on different hosting providers like Godaddy, BlueHost, and SiteGround.

### upload\_max\_filesize directive in php.ini. Godaddy

In Godaddy you can increase the max\_file size limit by editing the user.ini file. Once you get into the cpanel find the user.ini file or create one for yourself in the WordPress root directory.

In the user.ini file paste the following code

memory\_limit = 1024M  
max\_execution\_time = 180  
max\_input\_time = 180  
post\_max\_size = 64M  
upload\_max\_filesize = 720M

Pro Tip : max\_input\_time code is to maximize amount of time each script may spend parsing request data. It's a good idea to limit this time on productions servers in order to eliminate unexpectedly long running scripts.

### upload\_max\_filesize directive in php.ini. BlueHost

Login to your [BlueHost](https://www.bluehost.com/) cpanel, open the file manager and choose the WebRoot. On the right-hand side, you can see the php.ini file when you scroll. Right click on it and select the Code Edit.

Search for upload\_max\_filesize and give the value you need here it is 720M and the post\_max\_size as 64M that is

upload\_max\_filesize= 720M  
post\_max\_size = 64M

### upload\_max\_filesize directive in php.ini. SiteGround

[SiteGround](https://www.siteground.com/) gives you two options to edit your php.ini file one is their PHP variables manager tool and other is we have to manually edit the php.ini file as we have seen before. The tool is really handy for the beginners. Let’s see how to maximize file upload size using the tool.

[image of the SiteGround tool]

To edit the php.ini file using the PHP Variables Manager tool login to your cpanel and find the manager tool. Select the directory where WordPress is installed and click ADD.

In that, you will find the variables and the php fields that is the codes I explained above. In the appropriate field change the value you want and save the changes. If you want the changes to be set for all the sub-directories check the “Apply changes to all sub-directories” check box.

Note : this option is only available for the Cloud and dedicated hosting plans. For the Shared hosting you need to get the server side tech support.

## Ready To Increase Memory in WordPress Php.ini

These are the methods you can use to increase memory that is, increase the PHP memory. As like SiteGround most of the hosting provider will set their own PHP limits globally for the shared hosting. We cannot increase PHP memory in such server manually by ourselves. For that, we need to ask for the hosting provider support.

How you fixed the memory exhausted issue and increase memory in WordPress php.ini for the first time? Share your interesting experience below and if you need any help feel free to ask in the comment.